IFC building model
Schema: "IFC2X3"
File name: "Sample.ifc"
Time stamp: "12/11/2021 3:26:45 PM"
Preprocessor: "IfcOpenShell 0.5.0-dev"
Originating system: "IfcOpenShell 0.5.0-dev"
Application: "Klemen" version "v1.0" by Organization (no name given)

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Klemen" version "v1.0" by Organization (no name given) | change ADDED | created 1636024785 (2021-11-04T11:19:45Z) | last modified by Person (no name given) of Organization (no name given) with "Klemen" version "v1.0" by Organization (no name given)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "Unnamed1"
  IFCSITE "Default Site"
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey"
        contains 66 elements
          66 x IFCBUILDINGELEMENTPROXY | names: "ANSI_B27_7M_3CMI-4-46452_1", "SCREWS_60-60-30_1_2", "TULEJA_1_2_3_4_5_6_7_8_9_10_11_003" (+63 more) | property sets: Basic product data:, Dimensions:, Technical data:, Logistic data:, Manufacturer data:, Contacts:

Property sets
  Basic product data: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    Code: = "001102124" (IFCTEXT)
    Name: = "GT 60-60-30" (IFCTEXT)
    Product group: = "ETIBOX Distribution boards, metal enclosures and free-standing cable distribution cabinets" (IFCTEXT)
    Product link: = "https://www.etigroup.eu/products-services/001102124" (IFCTEXT)
    Short description: = "Enclosure, GT 60-60-30" (IFCTEXT)
  Dimensions: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    Depth (mm): = "300" (IFCTEXT)
    Height (mm): = "600" (IFCTEXT)
    Width (mm): = "600" (IFCTEXT)
  Technical data: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    Frequency (Hz): = "/" (IFCTEXT)
    Fusing characteristics: = "/" (IFCTEXT)
    IP Rating: = "IP66" (IFCTEXT)
    Number of poles: = "/" (IFCTEXT)
    Power dissipation (W): = "/" (IFCTEXT)
    Rated current (A): = "/" (IFCTEXT)
    Rated voltage AC (V): = "/" (IFCTEXT)
    Rated voltage DC (V): = "/" (IFCTEXT)
    Voltage type: = "/" (IFCTEXT)
    Weight (kg): = "22.99" (IFCTEXT)
  Logistic data: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    Basic packaging: = "1" (IFCTEXT)
    EAN (single product): = "3838895592013" (IFCTEXT)
  Manufacturer data: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    City: = "Izlake" (IFCTEXT)
    Country: = "Slovenia" (IFCTEXT)
    Manufacturer: = "ETI Elektroelement d.o.o." (IFCTEXT)
    Postal code: = "1411" (IFCTEXT)
    Street: = "Obrezija 5" (IFCTEXT)
    Website: = "https://www.etigroup.eu/" (IFCTEXT)
  Contacts: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    E-mail: = "support@eti.si" (IFCTEXT)
    Fax: = "00386 (0)3 / 56-74-077" (IFCTEXT)
    Telephone: = "00386 (0)3 / 56-57-570" (IFCTEXT)
  ETIM Classification v7.0: | properties | on 199 objects (132 (other), 66 IFCBUILDINGELEMENTPROXY, 1 IFCPROPERTYSINGLEVALUE)
    Built-in depth (mm): = "300" (IFCTEXT)
    Class name: = "Empty cabinet" (IFCTEXT)
    Classification: = "EC000058" (IFCTEXT)
    Colour: = "Grey" (IFCTEXT)
    Degree of protection (IP): = "IP66" (IFCTEXT)
    Depth (mm): = "300" (IFCTEXT)
    Height (mm): = "600" (IFCTEXT)
    Impact strength: = "IK10" (IFCTEXT)
    Material housing: = "Steel" (IFCTEXT)
    Mounting method: = "Surface mounted (plaster)" (IFCTEXT)
    Number of openings for flange plates: = "1" (IFCTEXT)
    Protection class: = "I" (IFCTEXT)
    RAL-number: = "7035" (IFCTEXT)
    Suitable for outdoor use: = "False" (IFCTEXT)
    Surface protection: = "Powder coating" (IFCTEXT)
    Transparent cover/door: = "False" (IFCTEXT)
    Type of door: = "Single" (IFCTEXT)
    Width (mm): = "600" (IFCTEXT)
    With lock: = "True" (IFCTEXT)
    With mounting plate: = "True" (IFCTEXT)